BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8902
CTI route timeout

This command is used to set the time during which the PBX waits for an automatic reroute position from a CTI telephony server.

##### Valid data

seconds | remark
1-30 |
4 | default up to R13
1 | default since R14

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005