BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2008
Verification tone on call back

The system supplies normal verification tone when it accepts an order. This can be altered so that silence is received instead.

##### Valid data

Yes |  | (verification) |
No |  | silence |

default data: YES

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005