BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x35
Invalid Card Number In Message

Default definition: |  | ERROR + TRIG |
Used by block: |  | ALL |
Category: |  | DESIGNER |

The card number in the message was not valid.

- D1: Received card position
- D2: Received INFCODE
- D3: Received SUBCODE
- D4: Received DATA+1

If ‘OS.WARNING code,DY’ is not used, data D3 and D4 are supplied by OS from the ME-register.

Revision: K © Ericsson Enterprise 2005