BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x17
Buffer Error

Default definition: |  | ERROR + TRIG |
Used by block: |  | OS |
Category: |  | DESIGNER |

Buffer error. The meaning of D2 depends on the value of D1.

D1 | Type of buffer error | D2 | Additionl data
01h | Data error (address) |  | Calculated buffer number
02h | Data error (buffer number) |  | Given buffer number
03h | Data error (link identity) |  | Given link ID
04h | Data error (not in chain) |  | Given link ID
05h | Data error (job ID) |  | Buffer job ID
06h | Data error (init) |  | Map number
10h | Buffer error (BUFFNUM) |  | Current buffer number
11h | Buffer error (BUFFLOG) |  | Current buffer number
12h | Buffer error (BUFFJID) |  | Current buffer number
13h | Buffer error (linked chain) |  | Current buffer number
14h | Buffer error (endless link) |  | Current buffer number
20h | Buffer handler (OSBUFF$QNT) |  | Current value
21h | Buffer handler (OSBUFF$FRE) |  | Current value
22h | Buffer handler (OSBUFF$BSY) |  | Current value
23h | Buffer handler (OSBUFF$LST) |  | Current value

- D3: Undefined
- D4: Undefined

Revision: K © Ericsson Enterprise 2005