BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1406
Wait time before ring back/rerouting at not answered calls

The command is used to determine the time before recall rerouting of unanswered incoming/transferred calls.

Value 0-255 seconds

The rerouting position is determined with commands 1103 Reroute position at day and 1104 Reroute position at night.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005