BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2408
Digit for Message

If a call is not answered or the called party is busy, the caller can enter the message system to send a message by dialling a suffix digit.

This command is used to determine the digit to be used for entering the message system.

If the digit has been used previously for another facility, it will be erased for this facility, i.e. the “old” facility will be removed from the system. See the other commands in this command group.

If a space is entered, access to the message system by post-dialling is removed.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005