BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0xDB
Feature Protected By FECU

Default definition: |  | ALARM + EXTERN + ACTIVE |
Used by block: |  | ALL |
Category: |  | MAINTENANCE |

An attempt to invoke a certain feature within the central software of ASB 150 02, or an attmpt to connect a specific hardware option to the exchange, was denied by the actual security level of the system. The programming of the current FECU (Feature Enabling Control Unit), connected to the front of the CPU-D4 central processor board, prohibits the execution of the feature or the activation of the hardware component.

- D1: ST, which rejects the execution of the feature
- D2: ID of the protected feature

- 00H ... Version 2.1 functionality of CTI.
- 01H ... Monitoring of operator instrument and queue.
- 02H ... Enhanced CIL functionality.
- 03H ... Tandem configuration with CTI.
- 04H ... Networking with QSIG.
- 05H ... Full networking (QSIG, VPN, UUS with MD 110).
- 06H ... Large / small scale networking.
- 07H ... ISDN caller list.
- 08H ... Enhanced individual abbreviated number.
- 09H ... Enhanced information system.
- 0AH ... GAP protocol.
- 0BH ... ACD - multiple call codes
- 0CH ... Swapping boards during operation
- 0DH ... Remote upgrading of central software
- 0EH ... Cordless remote O&M
- 0FH ... not used
- 10H ... UUI Italy
- 11H ... Adaptions for CN numbering plan feature
- 12H ... Alternative routing on no line available
- 13H ... Override number restriction in ISDN (Austria)
- 14H ... ISDN Point to Multipoint
- 15H ... Multiple incoming call presentation
- 16H ... ECE ISDN number translation
- 17H ... Austrian Call metering tariffs
- 18H ... VMU-HD individual greeting
- 19H ... Integrated MOH
- 1AH ... Fictive number extended / improved
- 1BH ... CN/operator services active
- 1CH ... CTI groups 8/16
- 1DH ... Very small networking (4 interfaces)
- 1EH ... X.25 protocol and X.31 services (packet mode terminals)
- 1FH ... UUI in Manufacturer Specific Information field of the Generic Functional Protocol
- 20H ... Conversation recording
- 21H ... Diversion individual to external destination
- 22H ... Integrated Cordless - GAP 2.0 protocol
- 23H ... Multiple music on hold
- 24H ... O&M - Remote FW upgrading
- 25H ... Very small Networking (2 interfaces)
- 30H ... Automatic summer / winter time change from ISDN
- 31H ... Verified Account Codes
- 32H ... 3-Party conference on ISDN
- 33H ... Call forwarding with partial re-routing
- 34H ...Centrex Hook Flash over ISDN
- 35H ...Outcall notification
- 36H ...Number translation
- 37H ...Leave ACD queue via exit position
- 38H ...Multi number redial
- 39H ...IP Extensions proprietary, IP Extensions H.323
- 3AH ... BusinessPhone VoIP Gateway
- 3BH ... Mobile Extension
- 40H ... Collect Call Blocking
- 80H ... Number of available voice channels exceeded or no final licence file applied within the 28 days temporary licence period.

- D3: Undefined, but if D2 = 80

- 01H ... no more voice channels are available
- 02H ... channels threshold for trunk calls exceeded
- 03H ... channels threshold for IP-client calls exceeded

- D4: Undefined, but if D2 = 80
  Currently used voice channels for the feature indicated in D3

#### Recommended action

If the warning occurs because of a new hardware component, added to the exchange, or if the customer has purchased the related functionality, connect the appropriate FECU to the CPU-D4 board.

Revision: K © Ericsson Enterprise 2005