BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4320
Notification scheduling profile

This command states which notification profile will be used to determine the waiting time after a non successfull call before the next attempt.

Following table shows the notification scheduling profile. There are 6 different profiles with different time tables.

profile | 1´st | 2´nd | 3´rd | 4´th | 5´th | 6´th | 7´th | 8´th | 9´th | 10´th
1 | 5 min | 10 min | 20 min | 40 min | 1h20min | 2h40min | 5h20min | 10h40min | na. | na.
2 | 10 min | 20 min | 40 min | 1h20min | 2h40min | 5h20min | 10h40min | na. | na. | na.
3 | 20 min | 40 min | 1h20min | 2h40min | 5h20min | 10h40min | na. | na. | na. | na.
4 | 30 min | 30 min | 30 min | 30 min | 30 min | 30 min | 30 min | 30 min | 30 min | 30 min
5 | 60 min | 60 min | 60 min | 60 min | 60 min | 60 min | 60 min | 60 min | 60 min | 60 min
6 | 90 min | 90 min | 90 min | 90 min | 90 min | 90 min | 90 min | 90 min | 90 min | 90 min

One Profile (1-6) have to be used, to notify the user, if a new incoming voice message arrives on his/her mailbox system. If the user does not answer with a key, the first notification will start 5 min later. If the user does not also notice the notification and does not press any key, the procedure will start with the second attempt. This procedure will go on, as soon as the user notice the notification to the 10´th attempt. After the last attempt the notification will be terminated.

Following table shows the limited resources to prevent a wrong configuration which will may be cause a decrease of the system resources.

max. amount of Users | min. allowed trunks | min. scheduling profile
5 | 1 | 1 (5 min, nonlinear)
10 | 2 | 1 (5 min, nonlinear)
20 | 2 | 2 (10 min, nonlinear)
30 | 4 | 2 (10 min, nonlinear)
40 | 6 | 3 (20 min, nonlinear
50 | 8 | 4 (30 min, linear)

Revision: E © Ericsson Enterprise 2005