BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0702
Client IP address

This command defines the IP-address of the IP-phone/IP-client, if the registration to the Gatekeeper shall only be allowed from a particular one.( e.g when free seating is not allowed ).

##### Valid data

0.0.0.0 - 255.255.255.255 |  |  |
0.0.0.0 (default) |  | registration is allowed from any IP-address |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005