BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1037
PNR routes at incoming proprietary call

This command states the number of PNR route choices which are allowed to be accessed at incoming proprietary calls to a PNR number. PNR alternative routing is performed when the called destination can not be reached over the first PNR route choice. If no more alternative route choice is available or allowed the call is released with reason ‘congestion’ and the previous proprietary PBX may perform alternative routing.

##### Valid data

Value = |  | 1 |  | route choice |
|  | 2 |  | route choices |
|  | 3 |  | route choices |
|  | 4 |  | route choices (initial value) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005