BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 44 E2RECORD

General communication with E2 handler.

For these messages an information code is used as subcode. The definitions here are made for extraction of subcodes for external files (Test-tool 'WILMER' and 'RASC'). All information codes are not valid for all three messages, see message descriptions for details.

E2BASRD |  | E2BASRD |
E2BASRL |  | E2BASRL |
E2BASSZ |  | E2BASSZ |
E2BASWR |  | E2BASWR |
E2RECRD |  | E2RECRD |
E2RECRL |  | E2RECRL |
E2RECSZ |  | E2RECSZ |
E2RECWR |  | E2RECWR |
E2RD |  | E2RD |
E2WR |  | E2WR |
E2BASSWAP |  | E2BASSWAP |
E2RECORD |  | E2RECORD |

EDh E2RECRDFST |  | Read first record linked to basic E2-record |
EEh E2RECRDNXT |  | Read next record linked to basic E2-record |
EFh E2BASPRMRD |  | Read programming model number of E2-base |
F0h E2BASPRMWR |  | Write programming model number of E2-base |
0F1h E2RECPRMRD |  | Read programming model number of E2-record |
0F2h E2RECPRMWR |  | Write programming model number of E2-record |
01h CERECCREATE |  | Indication for application blocks that CE has seized additional E2 record (contents only data converted by CE) |

Revision: F © Ericsson Enterprise 2005