BusinessPhone Communication Platform 7.0
Facilities

## IAS configuration tool

## Definition/Use

The IAS (Integrated Application Server) configuration tool is used for configuration, administration and maintenance of the IAS. It is self-contained, simple to install and use, and has a very wide range of configuration alternatives:

The IAS (Integrated Application Server) configuration tool is pre-installed on the IAS. Additionally is can be installed at the dealer/service centre premises or at the service technican PC.

## Operation

The IAS configuration tool can configure/maintain the following:

- IAS

- general and network settings
- start/stop of the IAS relevant services (BusinessLink, Directory Client, SUM server)
- Backup/restore of IP-phone configuration files, directory client, SUM server, BLink, BMS and BackStage

- BusinessLink

- For details pls. refer to BusinessLink (123/155 34-ASB 150 02 Uen)

- SumServer

- For details pls. refer to Slim Unified Messaging (465/155 34-ASB 150 02 Uen)

- Directory Client

- For details pls. refer to Alpha tagging via CTI (118/155 34-ASB 150 02 Uen)

- IP phone config file

## Connection principles

The IAS configuration tool is

1. pre-installed on the IAS.
2. additionally it can be installed at the dealer/service centre premises or at the service technican’s PC (for remote maintenance.

- If a firewall is between the IAS configuration tool and the IAS, then TCP - Port 9900 must be open

### IAS config tool on IAS

The pre-installed IAS configuration tool can be accessed by:

1. direct connection of monitor, keyboard and mouse to the IAS board
2. using a remote desktop connection. For download see http://www.microsoft.com/downloads/details.aspx?familyid=a8255ffc-4b4a-40e7-a706-cde7e9b57e79&displaylang=en

To see the background picture of the IAS - press Options - Experience and select LAN (make sure that desktop background is checked)

Note

If a firewall is between the remote desktop PC and the IAS, then TCP - Port 3389 must be open

### IAS config tool on any PC

A computer (PC) where the IAS configuration tool is installed can be locally or remotely connected to the IAS. The remote connection is done via the PBX's built-in V.32bis modem or via the internet

#### Local connection via V.24:

The services of the BusinessLink server and the IAS config server must be started

#### Local connection via IPU

The services of the BusinessLink server and the IAS config server must be started

#### Local connection via the LAN directly to IAS

The service of the IAS config server must be started

#### Remote connection via modem

The services of the BusinessLink server and the IAS config server must be started

#### Remote connection via the Internet and IPU

The services of the BusinessLink server and the IAS config server must be started

f

#### Remote connection via the Internet directly to IAS

The service of the IAS config server must be started

f

## Capacity

Number of systems, that can be configured/maintained by the IAS configuration tool is limited only by database capacity.

## Limitations & Programming

none

## Equipment

### ASB 150 02 system requirements

BusinessPhone Version 7.0 ( = ASB 150 02 R15 ) or higher.

### PC requirements

For the IAS configuration tool:

- Processor: Pentium 200 MHz
- Required hard disk space: 50 MB
- Minimum RAM available: 128 MB
- Operating systems

- MS Windows 2000 (Service pack 2 or higher)
- MS Windows XP (Service pack 1 or higher
- MS Windows 2003 server

Revision: A © Ericsson Enterprise 2005