BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8116
Mode digit display

Command 8103 Mode digit is used to determine whether a mode digit shall be sent to the paging equipment. ASB150 can only send single-digit mode digits.

The mode digits that are sent to the paging equipment have an important functional significance that depends on the different paging units available in the various markets.

Commands 8116 Mode digit display-8117 Mode digit speech are used to determine the mode digits to be sent for the different forms of alternative paging.

This command is used to determine the mode digit to be sent for display paging.

Range of values = 0-9

The function “display paging” can be removed from the system by writing over the mode digit with the space character.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005