BusinessPhone Communication Platform 7.0
Commands > Commands 4000...4999

## 4003
Answering time

This command is used to state the time for a call to be answered. If the operator does not answering a call within the stated time, the call will be rerouted to another operator or, if no other operator is on duty, to an alternative answering position. The PABX-operator is marked “off duty”.

Value = 15-255 s

##### Valid data

15-255 |  | s (default) |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005