BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0146
Meter info allowed on display?

The command defines whether or not own or other extensions shall have access to the extensions' metering information.

For all external calls metering information is stored in memory. The information then can be read (and displayed) e.g. by dialling procedure code *45# (accumulated metering information) or *46# (metering information for latest call). It is possible to read both metering information for own extension as well as metering information for other extensions.

In order to get access to a certain extension metering information, two parameters must be fulfilled:

- The calling party (calling e.g. *45#) must have an ACOS that permits access to own metering information or that of others. Note that there is one facility access command for reading “own” metering information (command 3075 Read own meter) and another command for reading metering information (command 3076 Read other’s meter) of others.
- The called party must permit (command 0146 Meter info allowed on display?) the metering information to be read.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005