BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8436
Carrier Name

This command allows to define and to store a name for a carrier in BusinessPhone 250/50. The name can have a maximum length of 20 ASCII code characters, while only eight different carrier (0-7) can be created. Only one name per carrier can be defined. It will only be used to display the carrier name on the O&M tool (BMS).

ASB 150 02 is only be used to store the carrier name in its memory.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005