BusinessPhone Communication Platform 7.0
Commands > Commands 0000...0999

## 0303
Ringing alternative

This menu shows the function of the programmable keys for the selected extension.

This command states the ringing type for presentation of incoming calls on the programmable key.

If the extension is busy when the ringing signal is to be sent, only one ringing period, muted even if the line is programmed as ringing, will be sent.

Note, that the ringinging alternative “direct answer” is only suitable for the key functions “ACD GROUP” and “INTERCOM” !!

##### Valid data

0 (default) |  | ringing |
1 |  | ringing after 10s |
2 |  | one muted ring |
3 |  | one muted ring/ringing after 10s |
4 |  | direct answer |

Minimum required authority level from telephone: 0

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005