BusinessPhone Communication Platform 7.0
Dialogs

## Trace Log

This dialog displays the contents of one of the six (0,1...5) trace logs.

The data in each log was saved when a TRACE-defined warning occurred. To interpret the data displayed by this function, a complete software source documentation is required.

Log number | Number of the log
Trace Log Header | Code, data and source (ST) from the warning.
Log date (from warning) | The date of the log, when the warning appeared.
Warning code | Click on the code link for more information.
Warning code data | Specific warning information.
Trace Selector A, (local) | First selector for the message trace extract.
Trace Selector B, (connected) | Second selector (if any) for the message trace extract.
Free Queue positions | For the message queues B,C and D
Free PCM Channels | total and for the common group
Message mask groups 1-3 | refers to the active masking when the log was saved.
Individual RAM (current) | if any, is the A-side (current process) individual ram
Individual RAM (connected) | If any, is the B-side (connected process) individual ram.
Process RAM | For the process.
Last Message | The last message prior to the warning.
Data | Related data
Extract from Message Trace | Is the data extracted from the message trace. If data matching the trace-selectors was found, only this data is extracted. Otherwise the latest data is extracted.

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |
Clear All |  | To clear all trace logs. |

See System Description (1551-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005