BusinessPhone Communication Platform 7.0
Dialogs

## Traffic Group Control

To access the dialog, open the “System” menu in the Configuration directory tree. Then open the “System facilities” submenu, click on “Traffic group” and select “Traffic group check” in the context menu.

The following commands are available:

Traffic Group Check

2340 |  | Traffic check at conference

2341 |  | Traffic check at operator conference

2342 |  | Traffic check at call pick-up

2343 |  | Traffic check at break-in

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To load the current system settings. |

See Facility Descriptions:

- Call Pick Up – Individual (144/15534-ASB 150 02 Uen).
- Conference (154/15534-ASB 150 02 Uen).
- Intrusion (267/15534-ASB 150 02 Uen).
- Operator (380/15534-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005