BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3303
Predigits

This command is used to define predigits, if any, for a normal route. The predigits are transmitted before the dialled external number.

Predigits = 1-10

The command is used to differentiate between variable and fixed numbering schemes. Normally, predigits need not be stated for variable numbering schemes. Predigits are to be stated for fixed number series.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005