BusinessPhone Communication Platform 7.0
Commands > Commands 9000...9999

## 9105
NPI for public calling/connected line identification

This command is used to define the Type Of Number (TON) for the public calling/connected line identification.

The following TON's are possible in accordance with the ISDN Network (E.164 number plan).

With R14 R3A or later the public CLI is sent/forwarded if 9101 Destination PBX = other vendor PBX and 9105 NPI for public calling/connected line identification is not Unknown (default)'

##### Valid data

International |  |  |
National |  |  |
Subscriber |  |  |
Unknown (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005