BusinessPhone Communication Platform 7.0
Commands > Commands 3000...3999

## 3201
Route members

This command states which trunks are to belong to a route and also the position of the trunk within the route.

A trunk is removed from a route by erasing the value of the relevant directory number.

Before this command can be executed, the command for creating route access codes (5401 Create a route) must have been executed.

On insertion of a trunk in a route the trunk is to be erased from its existing route (if one exists). This is of particular importance on installation when all trunks from the first BTU-card (without s-interface) will automatically be assigned to the route with call number 0.

##### Valid data

Trunk route directory number |  | Up to 46 trunks my be added to a route. A trunk may not belong to more than one route |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005