BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6017
Mode selection for serial interface

On the CPU-D4 central processor board the serial interface 2 can be switched between a RS-232 (V24) interface and RS-485 interface.The main purpose of the RS-485 interface is an increased line length of approximately up to 1000 m. Any other functional enhancements of the RS-485, combined with the RS-232 interface, are supported in the current release of the ASB 150 02. To fully configure a serial interface in ASB 150 02, also the commands 6006 Device type, 6007 Character set, 6009 Baud rate and 6010 Master/Slave respectively have to be defined.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005