BusinessPhone Communication Platform 7.0
Commands > Commands 5000...5999

## 5206
Login fail action

This command indicates the action to be taken by the PABX if too many consecutive invalid passwords have been received.

0 = No action |  |

1 = A warning is given. (This warning is normally entered in the alarm log of the PABX; see command group 74.) |  |

2 = The PABX is barred for login during a specified period of time. (Note that this barring does not comprise system programming from a system telephone, and that such programming can be permanently barred by entering the command 3003 System programming.) |  |

3 = The PABX is barred for login during a specified period of time. This barring comprises all calls, except extended calls and calls made after a recall. (System programming from system telephones is not barred; see above.) |  |

The barring time is set by means of command 5207 Login fail bar time.

Command 5205 Login fail limit determines the number of consecutive invalid passwords to be accepted before action is taken.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005