BusinessPhone Communication Platform 7.0
Warning Messages ASB 150 02 >

## 0x98
Invalid Warning Code Received

Default definition: |  | ALARM + EXTERN + ACTIVE + TRIG |
Used by block: |  | OM |
Category: |  | DESIGNER |

An invalid (out of range) warning code has been received by the OM programs. The original warning message is not changed, except for the code value, which is changed to W.OMINVWCODE.

- D1: Data from the original warning
- D2: Data from the original warning
- D3: Data from the original warning
- D4: Data from the original warning

Revision: K © Ericsson Enterprise 2005