BusinessPhone Communication Platform 7.0
Commands > Commands 9000...9999

## 9133
Predigits choice 3

This command is used to define predigits, if any, for the 2-nd route choice. The predigits are transmitted after the private network access code and before the dialled external number.

Predigits = 1-16.

Following commands for the 2-nd route choice will be ignored:

3302 Call back allowed |  |

3303 Predigits |  |

3304 Alternative route choice 1 |  |

3305 Predigits choice 1 |  |

3306 Alternative route choice 2 |  |

3307 Predigits choice 2 |  |

##### Valid data

0 - 24 |  | digits |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005