BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2029
Repetitive call-waiting tone

There are two ways for indicating call waiting towards analogue extension.

Value “no” gives a short tone each time a new call is put in the queue.

Value “yes” gives a continuos tone as long as there are calls waiting.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005