BusinessPhone Communication Platform 7.0
Dialogs

## H.323 Extension Gateway Data

Note

This feature is only available for BusinessPhone V5.1 (ASB 150 02 R13) or later versions!

The IP-Extension function is based on two components, a gatekeeper and an extension gateway, which are both located on the IPU board.

The IP-Extension function provides an integration of packet switched H.323 compliant clients, residing on a Local Area Network into the circuit-switched world of ASB 150 02.

The following commands are available:

2181 |  | H.323 Extension GK IP-address

2185 |  | H.323 Extension GW Q.931-port

For more information about a setting or a field, click on the command link in brackets to open the online help system. See also System Description (1551-ASB 150 02 Uen).

#### Actions

Submit |  | To submit your changes to the system. |
Reload |  | To reload the current system settings. |

### Other IPU Board Data dialogs

On top of the dialog, you find a navigation bar that provides access to the following IPU Board Data dialogs:

- Basic Data

- To go to the Basic IPU Data dialog.

- Ports

- To go to the Port configuration data dialog.

- Gatekeeper

- To open the Gatekeeper Data dialog.

- H.323 extension gateway data

- The dialog you view right now.

- H.323 trunk gateway

- To open the H.323 Trunk Gateway Data dialog.

- Licensing

- To go to the Voice Channel Licensing dialog.

- Board Configuration

- To open the Board Configuration dialog.

Revision: B © Ericsson Enterprise 2005