BusinessPhone Communication Platform 7.0
Commands > Commands 9000...9999

## 9147
Node reference 4

This command is used if the route choice is based on a VoIP connection. The IP address reference number refers to command 2186 Network Node reference. The following commands build the network node table: 2186 Network Node reference, 2163 Signaling protocol, 2164 Network IP address, 2187 Network Node Password).

##### Valid data

blank (default since R14) |  | not programmed |
0 (default up to R13) |  | the call set up is made with gate keeper assistance |
1-1000 |  | refers to command 2186 Network Node reference |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005