BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1955
MCID activation request allowed from TEs?

This command states whether MCID (Malicious Call Identification) is allowed by the terminal user(s) on the interface. A MCID request from terminal user is controlled before being sent to the T-interface.

##### Valid data

No |  | MCID is not allowed |
Yes |  | MCID is allowed |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005