BusinessPhone Communication Platform 7.0
Commands > Commands 9000...9999

## 9113
Predigits choice 1

This command is used to define predigits, if any, for the first route choice. The predigits are transmitted after the private network access code and before the dialled external number.

Predigits = 1-16.

Following commands for the 1-st route choice will be ignored:

3302 Call back allowed |  |

3303 Predigits |  |

3304 Alternative route choice 1 |  |

3305 Predigits choice 1 |  |

3306 Alternative route choice 2 |  |

3307 Predigits choice 2 |  |

##### Valid data

0 - 24 |  | digits |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005