BusinessPhone Communication Platform 7.0
Dialogs

## Tests

This dialog is used to give the user the ability to execute some tests.

#### Active Alarm Test

This function is used to verify that the programming and equipment for the ACTIVE ALARM function is correct. The programming is not affected.

The code for the active alarm test call will be W.OMACTIVE (= 9D) with data set to 00FF. Code 9D must be defined as 'ACTIVE'.

Remember that the test will not work if the port programmed for the active alarm function is used by BMS.

#### Heartbeat Test

This function is used to verify that the programming and equipment for the HEARTBEAT function is correct. The programming is not affected.

Remember that the test will not work if the port programmed for the heartbeat function is used by BMS.

#### Battery backed up RAM test

This function is used to test the integrity of the data in the battery backed up RAM. The same test is also run in the periodic (24hour) system internal test.

#### Battery backed up RAM recover

This function is used to recover areas in the battery backed up RAM.

Data that is marked as erroneous in this ram-area is removed and is lost. The areas occupied by the faulty data is marked as free, and can be used again.

Note

Data is stored as records in this memory. All data in a faulty record is lost.

#### Actions

Send Active Alarm Test Call |  | ... Start an active alarm test. |
Clear |  | … Start a heartbeat test. |
Start RAM Test |  | ... Start a battery backed up RAM test. |
Try RAM Recover |  | ... Start recovering areas of the battery backed up RAM. |

Revision: B © Ericsson Enterprise 2005