BusinessPhone Communication Platform 7.0
Commands > Commands 8000...8999

## 8003
Room to room open

It is possible to prevent calls between guests for a certain time during the 24-hour period.

The end time is determined with this command and the start time is determined with command 8002 Room to room bar.

The time must be stated in 24-hour format.

Range of values = 0-23 hours

The function can be removed by stating the same start and end times or by clearing the field.

Authorised extensions and telephone operators can also allow or bar calls between guests via a procedure (*34#). Command 3070 Block room to room / DID traffic is utilised to determine authorisation.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005