BusinessPhone Communication Platform 7.0
Facilities

## ISDN SS Terminal Portability (TP)

## Definition

The supplementary service TP enables the S-Interface user to interrupt ongoing communication, change the location of the terminal and thereafter reestablish the communication.

## Use

The S-Interface user can park the conversation partner (SUSPEND of call) for a max. of 3 minutes before the parked call must be reconnected again (RESUME of call). During this time can the S-interface user make a disconnection/re-connection of the terminal for a change of location (the terminal must be connected to on the same S-interface).

## Operation

See User Guide of the ISDN terminal.

## Capacity/Limitations

See User Guide of the ISDN terminal.

## Programming

See User Guide of the ISDN terminal.

## Equipment

BTU-B_ or MFU.

Revision: M © Ericsson Enterprise 2005