BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## BA VMSEIZANSW

0 VMACK |  | Seizure accepted |
1 VMRESACK |  | Reservation of a VMU-channel accepted |
2 VMNAKBUSY |  | Seizure rejected, channel busy |
3 VMNAKREF |  | Seizure rejected, reference error |
4 VMNAKCAP |  | Seizure rejected, capacity shortage |
5 VMNAKINS |  | Seizure rejected, card not installed |
6 VMNAKPROG |  | Seizure rejected, no reference for the dir.no |
7 VMNAKTO |  | Seizure rejected, time out (no VMU-answer) |
8 VMNAKBLK |  | Seizure rejected, no card or no time allocated |
9 VMNAKQ |  | Reservation not possible |

Revision: F © Ericsson Enterprise 2005