BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1007
Break-in allowed?

The command states whether intrusion shall be permitted during an ongoing call. However, intrusion is never permitted for data communications.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005