BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2274
Automatic Redial Answer Supervision Time

This command defines the time in seconds when the system is waiting for answer from a trunk in case of establishing an automatic redial.

Note

This parameter has to be set on a higher value than that was set by the trunk commands 1401 Number of digits with long dial supervision, 1402 Time supervision of long register sign. alt. MFC/MFE outgoing and 1403 Time supervision of short register sign. alt. MFC/MFE outgoing.
Otherwise unwished rescheduling of automatic redial will be happen.

##### Valid data

Valid values: |  | 15 - 255 seconds |
Initial values (default): |  | 60 seconds |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005