BusinessPhone Communication Platform 7.0
Installation Instruction ASB 150 02

## Marking Of Cables

Each cable that is connected to a PBX type ASB 150 should be marked on the cable’s designation holder with the label set SVH 277 003/4, supplied for this purpose. The cable TSR 902 0444/1 is supplied with a designation holder, 860 1839, at the EURO-connector.

This label set contains three label types:

Label 1: |  | This label indicates the abbreviated name for the PBA to which the cable is to be connected. Example of parameter:

Label 2: |  | There is one 2-digit parameter. This parameter indicates the position of the PBA-slot in the PBA where the cable is to be connected. Example of parameter:

Label 3: |  | There are two 1-digit parameters. The first parameter indicates the position of the pin-contact unit on the PBA. The second parameter indicates the 1/4 of the pin contact. Example of parameters:

These three labels indicate where the upper part of the cable is to be connected and are placed on the front side of the designation holder.

When the label 1 for PBA has a "_" included in the name, please enter the correct letter with a marker pen.

Revision: J © Ericsson Enterprise 2005