BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1039
Multiple Music on hold source number

The command defines the Music on Hold source number that is to be used by the trunk in case of an incoming call is parked, transferred or after the trunk announcement has been supplied to the external caller.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005