BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 0D MULTPRES

0 LEDCAD.FREE |  | Free indication, led off |
1 LEDCAD.BUSY |  | Busy indication, Continuous on |
2 LEDCAD.CALL |  | Call flash |
3 LEDCAD.PARK |  | Parking flash |
4 LEDCAD.CONN |  | Connected |
0 LEDCAD.OFF |  | Led off |
1 LEDCAD.ON |  | Continuous on |

Revision: F © Ericsson Enterprise 2005