BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6011
Autoselect allowed?

The command determines whether automatic selection of this port is allowed when locally connecting external equipment.

If the answer is no, the port will only be used by services which have commands of their own for selecting ports, for example command 6401 Initiate I/O ports for CIL.

If the answer is yes, the port may also be selected by services which have no command for the specification of ports, for example printout of the telephone directory (6502).

The I/O-port must also be programmed according to commands 6006 Device type, 6007 Character set, 6009 Baud rate and 6010 Master/Slave.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

In case of a CTI (with BusinessLink for Windows) connection the command must be set to NO (default value).

Revision: E © Ericsson Enterprise 2005