BusinessPhone Communication Platform 7.0
Dialogs

## Transfer To BusinessPhone

This function is used to transfer a complete offline configuration from the database to the system.

A configuration can be stored in the system only if the hardware configuration in the database and in the system are completely identical. Otherwise an error message will be displayed and the process will be terminated.

If there are directory number conflicts, BMS tries to resolve them by simulating writing to the system and searching for a sequence of write operations, so that the conflicts are avoided. If it is not possible to find such a sequence, an error message is displayed and the process is terminated.

If the data is not completely loaded and the background load is running, it will be automatically interrupted, before starting the transfer process.

While transferring the data, a progress indicator will be displayed.

When the transfer process is ready, this progress indicator will show:

Administrative Functions: My BP 3 [ONLINE] Ready

If the transfer fails, the progress/status indicator will show the corresponding information:

Administrative Functions: My BP 3 [ONLINE] Transfer to Exchange [E2 data]: 22% FAILED: Exception: Linked record could not be written. 112 CardST: 3; IndSN: 11; No: 50

If the user has cancelled the transfer, the progress/status indicator will show that the operation was interrupted by the user:

Administrative Functions: My BP 3 [ONLINE] Transfer to Exchange [E2 data]: 48% Interrupted by user

Attention:
If several versions of a backup exist, then always the latest is sent to BusinessPhone. In case, that an older version should be sent, the following has to be done:

- Load the desired old version
- ’Store’ the version (this action makes the loaded version to the latest
- Transfer to Exchange

See System Overview (1555-ASB 150 02 Uen).

Revision: B © Ericsson Enterprise 2005