BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1111
2nd, choice CN reroute position

The command is used to determine the 2nd. choice (of three possible) CN reroute position for the trunk. The programmable number refers to one of three system defined central answer positions. The value of the programmed reference number(s) defines also how the CN rerouting is handled.

- If no reference numbers are programmed at all for a trunk means this ‘CN rerouting not allowed or not available’.
- Programmed value 0 means that CN reroute destination number(s) are defined in the gateway PBX from where the rerouting will be executed.
- Programmed values 1-3 means that the system defined central answer position number(s) in accordance to commands 2077 First central answering position, 2078 Second central answering position, 2079 Third central answering position will be used for the CN rerouting.

Three attempts will be allowed in order to reach one of the 1st, 2nd and 3rd choice central answer position.

The order of priority for local and CN rerouting will be:

1. Local rerouting at day switched system
2. 1st choice CN rerouting
3. 2nd choice CN rerouting (1st coice is night switched)
4. 3rd choice CN rerouting (1st and 2nd choice is night switched)
5. Local rerouting at night switched system

Value ‘blank’, 0 , 1-3

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005