BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1040
Voice transmission quality

This command defines which voice transmission quality table (1-4) shall be used for gateway/transit call setups to an IP network, i.e. where any other type of trunk is the call originator towards an IP trunk. Each voice transmission quality table comprises a set of 4 codecs, whereby the access of the codecs relys on a different priority, which will be defined by the following commands:

2165 |  | Voice Transmission Quality Table 1

2166 |  | Voice Transmission Quality Table 2

2167 |  | Voice Transmission Quality Table 3

2168 |  | Voice Transmission Quality Table 4

##### Valid data

4 |  | Voice Transmisson Quality table |
2 (default) |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005