BusinessPhone Communication Platform 7.0
Signal Types, Internal Messages and CSW-Blocks > Internal Messages - Info Codes > Sorted by Info code

## 5E BLOCKINFO

01h BIOPTEMP |  | Time and temperature value |
02h BIPROTREQ |  | Request info about protection level |
03h BIPROTUPD |  | Inform about change in protection level |
04h BIRESCHKREQ |  | Request for a resource check |
05h BIRESCHKINIT |  | Initiate a resource check |
06h BIRESCHKRDY |  | Resource check has been finished |
07h BIKEYPADREQ |  | Request of ASCII characters programmed on the dedicated digit key |
08h BIKEYPADRSP |  | Response of ASCII characters programmed on the dedicated digit key |
09h BIKEYPADUPD |  | ASCII characters programmed on the dedicated digit key during preprogramming |
0Ah BIEXTMAIL |  | Broadcasts external voice mail address to operator |
0Bh BIDAYNIGHT |  | Information about the status of the system day/night switch |
0Ch BIDDICHGREQ |  | Request notification messages about DDI table changes |
0Dh BIDDICHGUPD |  | Receive notification messages with the DDI table changes |
00h PRTIDCTIV21 |  | Version 2.1 functionality of CTI |
01h PRTIDMONOP |  | Monitoring of operator instrument + queue |
02h PRTIDACCOUNTV24 |  | Enhanced CIL functionality |
03h PRTIDTANDEMCTI |  | Tandem configuration with CTI |
04h PRTIDNWQSIG |  | Networking with QSIG |
05h PRTIDNWFULL |  | Full networking |
06h PRTIDNWSMALL |  | Small scale networking |
07h PRTIDISDNCLIST |  | ISDN caller list |
08h PRTIDIAD |  | Enhanced individual abbreviated dialling |
09h PRTIDINFO |  | Enhanced information system |
0Ah PRTIDGAPPROT |  | GAP protocol |
0Bh PRTIDACDCCODES |  | ACD multiple call codes |
0Ch PRTIDSWAPBOARD |  | Swapping of boards during operation |
0Dh PRTIDUPGRADESW |  | Remote upgrading of central software |
0Eh PRTIDOMCORDL |  | Cordless remote O&M |
10h PRTIDUUIT |  | UUI Italy |
11h PRTIDCNNUMPLAN |  | Adaptation for CN numbering plan feature |
12h PRTIDALTROUT |  | Alternative routing on no line available |
13h PRTIDNUMREST |  | Override number restriction in ISDN (Austria) |
14h PRTIDISDNPMP |  | ISDN point to multipoint |
15h PRTIDMULTINC |  | Multiple incoming call presentation |
16h PRTIDDDITRANS |  | ECE DDI number translation |
17h PRTIDTARIFF |  | Austrian call metering tariff |
18h PRTIDPGREET |  | VMU-HD individual greeting |
19h PRTIDMOHIND |  | Integrated MOH |
1Ah PRTIDFNENH |  | Fictive numbers extended/improved |
1Bh PRTIDCOPACT |  | CN/operator services active |
1Ch PRTIDCTIGRP816 |  | CTI groups 8/16 |
1Dh PRTIDNW4 |  | Very small networking (4 interfaces) |
1Eh PRTIDX25X31 |  | X.25 protocol and X.31 services (packet mode terminals) |
1Fh PRTIDUUIGPF |  | UUS in MSI of GPF |
20h PRTIDCONVREC |  | Conversation recording |
21h PRTIDIED |  | Diversion individual to external destination |
22h PRTIDGAP20 |  | Integrated Cordless – GAP 2.0 protocol |
23h PRTIDMULTMOH |  | Music on hold (1 integrated and 7 external sources or 8 external sources) |
24h PRTIDUPGRADEFW |  | O&M – Remote FW upgrading |
25h PRTIDNW2 |  | Very small networking (2 interfaces) |

Revision: F © Ericsson Enterprise 2005