BusinessPhone Communication Platform 7.0
Commands > Commands 1000...1999

## 1972
Call Forwarding with Partial Rerouting is subscribed

The command is used to define, if Call Forwarding (CF) with Partial Rerouting (PR) is subscribed or not from the network operator for the current ISDN-link.

That states, if any reroute facility request (with reason CFU/CFB/CFNR) is allowed to be sent to the network, which it is, if subscribed.

##### Valid data

NO (default) |  | Call Forwarding with Partial Rerouting facility is not subscribed |
YES |  | Call Forwarding with Partial Rerouting facility is subscribed. |

Note

This command is programmable only for T-interface !

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005