BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2142
GK Backup NGK RAS transport address

For each of the in command 2140 GK Primary NGK RAS transport address specified NGKs the RAS transport address of a Backup-NGK can be specified. This address is used in case of the Primary-NGK is out of order.

##### Valid data

|  | Network IP address |  | Port number |
1-25 |  | 0.0.0.0 - 255.255.255.255 |  | 0-65535 |
1-25 |  | 0.0.0.0 (default) |  | 1719 (default) |

Note

The RAS Port number of an gatekeeper in ASB 150 02 R14 is fixed to 1719

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005