BusinessPhone Communication Platform 7.0
Commands > Commands 2000...2999

## 2105
Minimum release signal

A break in the loop from analogue extension telephones can be interpreted either as a digit pulse or a register access signal or a release signal, depending on the type of telephone, connection case and length of the break.

Command 2105 is used to state the shortest break that must always be interpreted as release signal for analogue extensions. The time is stated in units of 10 ms.

10 = |  | 100 ms

11 = |  | 110 ms

. |  |

. |  |

. |  |

99 = |  | 990 ms

Breaks shorter than this time can be interpreted as a register access signal or rotary dial pulse.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: J © Ericsson Enterprise 2005