BusinessPhone Communication Platform 7.0
Commands > Commands 6000...6999

## 6432
Enable test protocol

This command is used to enable or disable the IO port specified in command 6431 Test protocol port address to be used for the ASB 15002 test protocol. The test protocol is used for the PC Operator V1.x or for the test tool software.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: YES

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2005