BusinessPhone Communication Platform 7.0
Commands > Commands 9000...9999

## 9101
Destination PBX

The dialled private network access number will associated to ‘type of corporate network call’, parameter indicating if call setup destination is ‘proprietary PBX’ (BP.MD) or ‘other vendor PBX’.

If destination is ‘proprietary PBX’ the type of network call is ‘proprietary corporate network call’ or ‘other vendor PBX’ then type of network call is ‘non-proprietary corporate network call’.

This information is used to activate/deactivate proprietary services for the started call setup.

With R14 R3A or later:

If 9101 Destination PBX = other vendor PBX AND 9105 NPI for public calling/connected line identification is not Unknown, then the CLIP information is arranged based on:

2236 |  | Own country code

2237 |  | Own area code

2220 |  | Public number

2224 |  | Type

1030 |  | Public number group

If 9101 Destination PBX = other vendor PBX AND 9105 NPI for public calling/connected line identification is Unknown (default), then the private CLIP information is sent.

##### Valid data

0 |  | proprietary PBX |
1 |  | other vendor PBX |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2005